[](http://www.mkey.com.au/) Garage Remote Control Programming Instruction

[](http://mkey.com.au/remote,298,,forzablue,forzablue#1)[](http://mkey.com.au/remote,280,,Forza_silver,forza_silver#1)

Forza Silver/Blue/1000/2000

***Step 1***: Open the cover of Forza opener by pressing the dark red button on the door opener unit

***Step 2***: Inside the opener, you will see the receiver board, press and release **S1/LEARN** (program) button on the board 🡺 Red LED will be on

***Step 3***: Then press any desired button on the new remote for 1 second then release 🡺 Red LED will start flashing then extinguish

***Step 4***: Programming is complete. Press the button to test whether it works 🡺 If no success, repeat the above step 2&3.

► If you use the remote to operate **main entry gate/door** of block of unit/apartment:

* you will first need to locate the receiver box (left picture below) which is usually attached to the motor (middle picture)
* the **S1** (program) button is on the circuit board inside (right picture)
* following the above step 2&3 to program the new remote

