**Set the security code**

The security code • dip' switches or • rolling' switch are located behind the snap off cover on the right hand side of the motor head.

* Dip switches(if applicable)

The 12 switches are pre - set in the factory in the • on' position. Set the switches in a random pattern of your choice. The switches in the hand trans­mitter are located under the battery cover on the back of the transmitter. Set the switches to correspond with patterns in the motor head.

* Rolling switches(if applicable)

The security code • rolling' switch should be operated as follows:

1. Press and release black programming button located on receiver board. (Red Pilot light will begin to flash) .

2. Press hand transmitter button for 1 sec and then release. (Red pilot light will stop flashing) .

3. Press hand transmitter button for another 1 sec and then release. (Red pilot light will flash for approximate 3 sec) .

4. When red pilot light stops flashing the programming sequence is com­plete. To program additional transmitters repeat steps 1-5.

Deleting stored codes: Your security code system will store up to 7 trans­mitter codes. If more than 7 transmitters are programmed, the system will systematically start to delete the previously programmed transmitter. (i. e. transmitter 8 is programmed then No.1 will drop out. If 8, 9, 10 are pro­grammed the 1,2, 3 will drop out etc. )

To delete all stored codes: Simply press and hold the programming but­ton, red pilot light will come on. When red pilot light switches off, all pre­viously programmed transmitters will have been deleted.