***Boss 2211-L Transmitter instruction***

***Thank you for purchasing from us.***

***Programming the transmitter code into the drive unit to activate***

***1. Push RADIO SET BUTTON at the back of drive unit –Courtesy light will come on.***

***2. Push handset button you wish to operate the door. Courtesy light will flash twice***

***3. Now test by pressing the button on the transmitter.***

***Deleting all transmitter codes***

***1. Hold RADIO SET BUTTON in for 5 seconds, All memories of your remotes (include***

***lost remotes) will be deleted – Courtesy light will flash 7 times.***

***2. Test by pressing Button on a previously coded transmitter-the motor should not***

***respond.***

[***www.magickey.com.au***](http://www.magickey.com.au/)